(footprint "SolderJumper-3_P2.0mm_Open_TrianglePad1.0x1.5mm_LTR_PlusMinus"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open, labeled with numbers")
	(tags "solder jumper open")
	(property "Reference" "REF**"
		(at 0.725 -1.775 0)
		(layer "F.SilkS")
		(uuid "1f0d5fe8-a5df-49bf-a2eb-d8afb90a5183")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SolderJumper-3_P2.0mm_Open_TrianglePad1.0x1.5mm_LTR_PlusMinus"
		(at 0.725 1.925 0)
		(layer "F.Fab")
		(uuid "5a5bfa3a-68e4-4a9c-8268-44da94e5e21e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0eabb3a4-c21f-4e35-8b72-7dc99af7b861")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "45fd55dd-5699-467b-bdb9-dedd06137ed3")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(zone_connect 1)
	(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
	(fp_rect
		(start -2.5 -0.75)
		(end 2.5 0.75)
		(stroke
			(width 0)
			(type default)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "7ecf8b53-f22f-436c-a433-7b3655bd3320")
	)
	(fp_line
		(start -2.75 -1)
		(end 2.75 -1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d16ace72-fc89-492a-9ce6-6ffdf0a8db43")
	)
	(fp_line
		(start -2.75 0.95)
		(end -2.75 -1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "861951cd-a9d4-44bd-9506-75f91d4fe370")
	)
	(fp_line
		(start 2.75 -1)
		(end 2.75 0.95)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f09a1c58-4451-4234-860a-a4e578fcb034")
	)
	(fp_line
		(start 2.75 0.95)
		(end -2.75 0.95)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "99cf9435-3b7a-457b-9ab8-596eaa71627a")
	)
	(fp_line
		(start -2.98 -1.27)
		(end -2.98 1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9e9be06c-d900-4f07-95da-50219e19050e")
	)
	(fp_line
		(start -2.98 -1.27)
		(end 3 -1.27)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "cfd3c5f0-b06c-40df-9f8c-7e0303b1448a")
	)
	(fp_line
		(start 3 1.25)
		(end -2.98 1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c408155c-c777-45f5-b0c9-84f58b19b403")
	)
	(fp_line
		(start 3 1.25)
		(end 3 -1.27)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c87e9f8b-2917-4ce9-a719-65807c416b7c")
	)
	(fp_text user "+"
		(at -3.35 0 0)
		(layer "F.SilkS")
		(uuid "ae98f1f5-0537-4aa5-a7b9-0a30745d82bd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "-"
		(at 3.4 0 0)
		(layer "F.SilkS")
		(uuid "cd5bf73d-d9e9-4524-8dea-462756c7651b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd custom
		(at -2 0)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1 0) (xy 0.5 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0.5 -0.75)
				)
				(width 0)
				(fill yes)
			)
		)
		(uuid "20250216-b954-4d07-8b54-6a6e0b8f3775")
	)
	(pad "2" smd custom
		(at 0 0)
		(size 0.3 0.3)
		(layers "F.Cu")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.2 0) (xy 0.7 0.75) (xy -1.2 0.75) (xy -0.7 0) (xy -1.2 -0.75) (xy 0.7 -0.75)
				)
				(width 0)
				(fill yes)
			)
		)
		(uuid "26a0ae10-67fb-4733-91e4-512cabf72010")
	)
	(pad "3" smd custom
		(at 2 0 180)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.5 0) (xy 1 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 1 -0.75)
				)
				(width 0)
				(fill yes)
			)
		)
		(uuid "b63fa587-bec2-494a-a9e5-0548e6c28061")
	)
	(embedded_fonts no)
)
