(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "SolderJumper_3_Open_ArrowPlusMinus"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom no)
		(on_board yes)
		(property "Reference" "JP7"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "CS TFT"
			(at 0 6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Project_Library:SolderJumper-3_P2.0mm_Open_TrianglePad1.0x1.5mm_LTR_PlusMinus"
			(at 0 -2.794 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "~"
			(at 1.016 1.778 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 2.794 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Solder Jumper SPDT"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "SolderJumper*Open*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "SolderJumper_3_Open_ArrowPlusMinus_0_1"
			(polyline
				(pts
					(xy -2.54 0) (xy -2.032 0)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -1.27 1.27)
				(mid -1.27 1.27)
				(end -1.27 1.27)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -1.27 1.27)
				(mid -1.27 1.27)
				(end -1.27 1.27)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.016 1.016) (xy -0.508 0) (xy -1.016 -1.016)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(arc
				(start -1.016 -1.016)
				(mid -2.032 0)
				(end -1.016 1.016)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -0.508 -1.016) (xy 0 0) (xy -0.508 1.016) (xy 0.508 1.016) (xy 1.016 0) (xy 0.508 -1.016) (xy -0.508 -1.016)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -1.27) (xy 0 -1.016)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.016 1.016) (xy 1.524 0.762) (xy 1.778 0.508) (xy 2.032 0) (xy 1.778 -0.508) (xy 1.524 -0.762)
					(xy 1.016 -1.016) (xy 1.524 0) (xy 1.016 1.016)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(arc
				(start 1.016 1.016)
				(mid 2.032 0)
				(end 1.016 -1.016)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.016 -1.016) (xy 1.524 0) (xy 1.016 1.016)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0) (xy 2.032 0)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "SolderJumper_3_Open_ArrowPlusMinus_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
)
